Bottom weight module recess too small (5)

3 washer under the bottom

¼ -->⅛ (9)

Through hole larger

Longer through bolt >3