Phototransistor: Up F1 FrontR F4 FrontL F5 RearR F6 RearL F7

R motor: PWM B6 Dir B3 OCR1B

L motor: PWM B7 Dir B2 OCR1C

Light: Small Y B4 B5: Side A or B

Small B C6 C7: Go for the goal or puck

Small W D3: Catch or not

Large RGB D5 D6 D7

Switch: Side B0 Light B1

M\_red: Flash one time : Receive wireless signal one time

M\_green: On: Play